#
# Logscale axis tic placement has always been problematic.
# This demo exercises both automatic tic placement and
# user-specified tic series.
#
set log y
set log y2
set tics nomirror
set border 11
set key center title "rangelimited tics" samplen -1

set xrange [1:15000]

set ytics 10 logscale rangelimit
set y2tics auto rangelimit

plot sample [x=2:14000] x axes x1y1 title "set ytics 10", \
            [x=2:14000] x axes x1y2 title "set y2tics auto"

pause -1 "<cr> to continue"
reset
